
**Hands-on Lab**

**Lego NXT – NXT Motor Open-Loop Step Response (OLSR)**

In class, the theory underlying a DC motor was presented. Briefly, a DC motor can be modeled as a first order system. Here, a step input (i.e. a constant voltage) is applied to the motor. The motor’s rotational speed gradually reaches a steady-state value as depicted in **Figure 1** below. This lab demonstrates this phenomenon. CountTick is used to set the sampling time, and to calculate the time between changes in the motor’s angle. The resulting speed (rad/s and RPM) are computed and saved as a file. XLS scatter plot (Figure 1 graph) shows the motor’s first-order response.



**Figure 1**: Open-Loop Step Response of a LEGO NXT motor

**Step 1**: Write save, and compile **motorOlsr1\_0a.nxc**

Note: The program is long only because it is filled with comments. Moreover, the code leverages the concepts learned in file handling (e.g. x^2File1.0.nxc) and timers (e.g. stopWatch1\_0a.nxc).

// File: displaySquareAndSquareRoot3\_0.nxc

// FILE: mtrOlsr1\_0a.nxc - Works!

// AUTH: P.Oh

// DATE: 03/13/23 15:58

// DESC: OLSR of NXT motor (Port A) with data written to file olsr.csv

// with 40 msec sampling time

// VERS: 1\_0a: ME 425/625 Release version

// REFS: nxtMotorOlsr1\_0.nxc; x^2File1.0.nxc, rotate0\_1a.nxc, mtrSpeed0\_2a5.nxc

// mtrOlsr0\_1a.nxc

// NOTE: Uses MotorRotationCount which reports encoder count in degrees

// and program calculates difference over delta tic counts

#define MOTOR OUT\_A // set constant MOTOR for Port A

#define FULL\_SPEED 75 // 75 percent of possible motor speed

#define DEG2RPM 166.667 // deg/msec to RPM

#define RPM2RADPERSEC 0.105; // RPM to rad/sec

task main() {

// Declare variable -----------------------------------------------------

// Motor related variables

long degPrev, degCurr, degDelta; // motor's degrees previous,current, delta

float motorRpm; // motor speed [RPM]

string strMotorRpm; // string form of motorRpm

float motorRadPerSec; // motor speed [rad/s]

string strMotorRadPerSec; // string form of motorRadPerSec

// File related variables

unsigned int result; // flag returned when handling files

byte fileHandle; // handle to the data file

short bytesWritten; // number of bytes written to the file

string fileName, fileHeader, text; // name, header and text to write to file

// Timing related variables

long ticPrev, ticCurr, ticDelta; // previous, current and delta ticks

long ticWait, ticEnd; // ticks to wait and to end

long msSamplingTime; // sampling time in [msec]

float secElapsed; // seconds elapsed in [sec]

string strSecElapsed; // string form of secElapsed

// Button related variables

bool orangeButtonPushed, rightArrowButtonPushed;

// Initialize variables --------------------------------------------------

secElapsed = 0.0; // set elapsed time to zero

degPrev = 0; // motor initially motionless so set angle to zero

msSamplingTime = 40; // [msec] sampling time

// Algorithm starts here ---------------------------------------------------

// (1) Set up the file

fileName = "olsr.csv" ; // <---- file name you want data saved to

result=CreateFile(fileName, 2048, fileHandle);

// (1A) Check if filename already exists, and overwrite it

while (result==LDR\_FILEEXISTS) {

CloseFile(fileHandle);

DeleteFile(fileName);

// result=CreateFile(fileName, 1024, fileHandle);

result=CreateFile(fileName, 2048, fileHandle);

} // end while

// (1B) write column header to file

fileHeader = "Time [s], RAD/S, RPM" ; // <---- column header in your CSV file

WriteLnString(fileHandle, fileHeader, bytesWritten);

// (2) Process that generates data

// Prompt user to begin step input

TextOut (0, LCD\_LINE1, "-> starts" );

do { // wait until user hits right button

rightArrowButtonPushed = ButtonPressed(BTNRIGHT, FALSE);

} while(!rightArrowButtonPushed);

// Begin step response

TextOut (0, LCD\_LINE1, "Orange Btn quits" );

strSecElapsed = FormatNum("%5.3f" , secElapsed);

// (2A) read current motor angle [deg] and poll timer before applying power

degPrev = MotorRotationCount(MOTOR);

// Command motor to move i.e. step input

ticPrev = CurrentTick(); // poll timer 1st time <<<<<<<<<<<<<<<<<<<<<<<<<<<

OnFwd(MOTOR, FULL\_SPEED); // turn on motor at FULL\_SPEED value

do {

// (2B) poll timer a 2nd time, measure elapsed time in [msec], read

// motor's rotational angle [deg] and compute rotational speed [RPM]

ticCurr = CurrentTick(); // poll timer a 2nd time <<<<<<<<<<<<<<<<<<<<<<<<<

// Read change in motor angle

degCurr = MotorRotationCount(MOTOR); // get relative position [deg]

degDelta = degCurr - degPrev;

// Measure elapsed time and hence motor RPM

ticDelta = ticCurr - ticPrev; // time [msec] elapsed between angle reads

motorRpm = (degDelta \* DEG2RPM) / ticDelta; // deg/ms \* DEG2RPM yields RPM

strMotorRpm = FormatNum("%5.2f" , motorRpm);

// Display motor actual speed and elapsed time

TextOut(0, LCD\_LINE4, FormatNum("RPM = %5.2f" , motorRpm));

TextOut(0, LCD\_LINE6, FormatNum("Time = %5.3f s" , secElapsed));

// (2C) compute rotational speed [rad/s]. Form string versions of the data

// and write to file

motorRadPerSec = motorRpm \* RPM2RADPERSEC; // RPM \* RPM2RADPERSEC gives rad/s

strMotorRadPerSec = FormatNum("%5.3f" , motorRadPerSec);

secElapsed = secElapsed + (ticDelta/1000.0); // [sec]

strSecElapsed = FormatNum("%1.2f" , secElapsed);

text=StrCat(strSecElapsed, "," , strMotorRadPerSec, "," , strMotorRpm);

WriteLnString(fileHandle, text, bytesWritten);

// (2D) call the current values the previous ones before looping back

ticPrev = ticCurr; // assign 2nd polled tick value to 1st polled tick value

degPrev = degCurr; // assign current rot'n count as previous rot'n count

// (2E) compute how much time to do nothing until sampling cycle is completed

// EG: suppose the current loop iteration took 35 msec. Suppose the defined

// sampling time is 40 msec. Thus, we should wait for 5 msec before looping

// back.

ticEnd = CurrentTick(); // <<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<<

ticWait = msSamplingTime - (ticEnd - ticCurr);

Wait(ticWait);

// Check if user wants to quit

orangeButtonPushed = ButtonPressed(BTNCENTER, FALSE);

} while( !orangeButtonPushed );

// Orange button pressed, so command 0 speed to motor and quit

ClearScreen();

TextOut(0, LCD\_LINE2, "Quitting", false);

// Stop motor

OnFwd(MOTOR, 0);

CloseFile(fileHandle);

PlaySound(SOUND\_LOW\_BEEP); // Beep to signal quitting

Wait(SEC\_2);

StopAllTasks();

} // end of main

**Program:** **motorOlsr1\_0a.nxc**

**Step 2**: Construct a mount for your LEGO NXT motor. Connect the motor to Port A on the Brick. Execute motorOlsr1**\_0a.nxc**. This will immediately have the NXT motor (that’s connected to Port A) move at 75% power. Count 3 to 5 seconds, and then press the Orange button. This will stop the motor and quit the program.

**Step 3:** Refer to Concept 1 in the Lab entitled **labBricxxFileHandling-102822a.pdf**. Recall, one can use BrixCC’s Tools- NXT Explorer to see the files in one’s Brick. Click and drag the file olsr.csv to your laptop. Use Excel to open the file and create a scatter plot (like the one shown above in Figure 1).

**Code Explanation**: The cyan highlight of Step (1) is very similar to the code in x^2File1\_0.nxc. This section creates a file named olsr.csv and writes a comma separated header for 3 columns of your data: Time [s], RAD/S, and RPM. Recall, Excel reads CSV files and will automatically put any data in these columns for easy plotting.

Step (2A) reads the motor’s current angle [deg], polls the timer with a CountTick, and then applies power to the NXT motor. Step (2B) begins the do-while loop. Here, one polls the timer and reads the current motor angle. Step (2C) uses that information to compute the motor’s rotational speed and writes the data to the file.

Highlighted in green is Step (2E). This is important to ensure the desired sampling rate. In other words, one wants to sense, compute, and write data at specific times (i.e. at the sampling rate). The comments give an example to rationalize the need for Step (2E). Here’s another example. One observes the program has two TextOut statements. These display the motorRpm and secElapsed on the Brick. Displaying info is a time-consuming process for any micro-controller. For the NXT, such displays can take 2-5 milliseconds to execute. Also, the do-while loop has a single WriteLnString function. This also consumes time, but varies. Some microprocessors collect data to write into RAM and then flushes it to memory (e.g. EEPROM) when it’s filled. Other microprocessors write data directly to memory. Some microprocessors do a combination. The net effect is that Step (2E) employs a Wait statement to ensure the do-while loop time matches the prescribed sampling time.

**Exercise 1:** In NxC create programs for the following:

* 1. Repeat **motorOlsr1\_0a.nxc** but using (1) a 25% and (2) 50% power level. Compare the resulting open-loop step response plots with the 75% power level. What are the rise times for the 3 different plots? Why are they different or the same?